**1.1 Safety regulations**

The following safety regulations must be observed at all times:

* The meter connections must be disconnected from all voltage sources before installing the module.
* Contact with live parts can be fatal. The main fuses should, therefore, be removed and kept in a safe place until the work is completed so that other persons cannot replace them unnoticed.
* Local safety regulations must be observed. Only technically qualified and appropriately trained personnel are authorised to install the modules.
* Only appropriate tools shall be used for the job. This means, e.g. that the screwdriver must be of the correct size for the screws, and the handle of the screwdriver must be insulated.
* Modules must never be cleaned under running water or with com­pressed air. Water ingress can cause short-circuits or damage elec­tronical components.